**DRAFT CREATED By: BD 02-08-2021**

**OAR 581-053-0240 Minimum Standards for School Buses**

**(Excerpt)**

(71) Stop Signal Arms: Buses shall be equipped with stop signal arms mounted in accordance with the following requirements:

…

(b) A wind guard or mechanism defaulting the stop signal arm to a retracted state when not activated shall be provided. All sheet metal parts shall be 16-gauge metal or heavier;

Statutory/Other Authority: ORS 327.013 & 820.100 - 820.120

Statutes/Other Implemented: ORS 327.013, 820.100, 820.105, 820.110 & 820.120

History:

ODE 5-2018, amend filed 02/21/2018, effective 02/21/2018

ODE 40-2014, f. & cert. ef. 9-3-14

ODE 19-2012, f. & cert. ef. 6-14-12